**Table A1** Numerical simulations of wellbore flow and heat transfer in SC-CO2 fracturing

|  |  |  |  |  |  |  |  |
| --- | --- | --- | --- | --- | --- | --- | --- |
| Fracturing technology | Well type | Heat transfer medium | Heat source | Friction coefficient | Heat transfer and flow state | Heat transfer description method between CO2 and formation | References |
| Tubing  fracturing | Vertical well | CASF | Joule–Thomson effect | Chen (1979) | Steady & steady | Comprehensive heat transfer coefficient | Dou et al. (2013) |
| CTACSF | Friction heat | Chen (1979) | Unsteady & unsteady | Differential equation | Guo and Zeng (2015) |
| CTACSF | Joule–Thomson effect & friction heat | U | Unsteady & unsteady | Differential equation | Guo et al. (2015) |
| CASF | N | Jain (1976) | Unsteady & steady | Comprehensive heat transfer coefficient | Lv et al. (2015) |
| CTACSF | Joule–Thomson effect & friction heat & expansion/compression work | Wang et al. (2014) | Steady & steady | Comprehensive heat transfer coefficient | Li et al. (2018) |
| CTACSF | Joule–Thomson effect & friction heat | U | Unsteady & unsteady | Differential equation | Lyu et al. (2018a) |
| CTACSF | Joule–Thomson effect & friction heat | Chen (1979) | Unsteady & unsteady | Differential equation | Lyu et al. (2018b) |
| CTACSF | Friction heat | Wang and Touber (1991) | Unsteady & unsteady | Differential equation | Yang et al. (2018a) |
| CTACSF | Friction heat | Churchill (1977) | Steady & steady | Comprehensive heat transfer coefficient | Yang et al. (2018b) |
| CTACSF | Joule–Thomson effect | Wang et al. (2014) | Steady & steady | Comprehensive thermal resistance | Bai et al. (2019) |
| CTACSF | Joule–Thomson effect & friction heat | U | Unsteady & unsteady | Differential equation | Gong et al. (2019a) |
| CTACSF | N | Wang et al. (2014) | Unsteady & unsteady | Differential equation | Wang et al. (2019a) |
| Horizontal well | CTACSF | Joule–Thomson effect & friction heat | Zheng et al. (2017) | Unsteady & unsteady | Differential equation | Lyu et al. (2021) |
| Tubing and annulus  co-injection fracturing | Vertical well | CTACSF | Joule–Thomson effect & friction heat | Chen (1979) | Unsteady & unsteady | Differential equation | Gong et al. (2019b) |
| CTACSF | Joule–Thomson effect & friction heat & expansion/compression work | Chen (1979) | Unsteady & unsteady | Differential equation | Wu et al. (2021) |
| Coiled tubing  jet fracturing | Vertical well | CASF | N | U | Steady & steady | Comprehensive heat transfer coefficient | Cheng et al. (2014) |
| CTACSF | N | Wang et al. (2014) | Steady & steady | Heat transfer quantity for each medium | Song et al. (2017) |
| CTACSF | Friction heat | Churchill (1977) | Steady & steady | Comprehensive heat transfer coefficient | Yang et al. (2018c) |
| CTACSF | Joule–Thomson effect & friction heat | Churchill (1977) | Unsteady & unsteady | Differential equation | Yi et al. (2019) |

Note: CASF- Carbon dioxide, annulus, cement sheath, and formation, CTACSF- Carbon dioxide, tubing, annulus, casing, cement sheath, and formation, N- No, U- Unknow.

**Table A2** Numerical simulations of fracture initiation and propagation in SC-CO2 fracturing

|  |  |  |  |  |  |  |  |  |  |  |
| --- | --- | --- | --- | --- | --- | --- | --- | --- | --- | --- |
| Method | Coupling | CO2 compressibility | Rock heterogeneity | Propagation criteria | Reservoir | Weak plane | Dimension | Physical model size (m) | Solution software/code | References |
| DEL | HM | Y | Y | Stress intensity factor K1 | Shale | N | 2D | 0.1×0.1 | COMSOL&MATLAB | Zhang et al. (2017a) |
|
| HM | Y | Y | Maximum tensile stress criterion & Mohr-Coulomb criterion | Shale | N | 2D | 1.9×1.9 | COMSOL&MATLAB | Liu et al. (2018) |
| THM | Y | Y | Maximum tensile stress criterion & Mohr-Coulomb criterion | Tight sandstone | N | 2D | 2×2 | COMSOL | Zhang et al. (2018) |
| HM | Y | Y | Maximum tensile stress criterion & Mohr-Coulomb criterion | Shale | Bedding planes | 2D | 0.2×0.2 | COMSOL&MATLAB | Zhang et al. (2019) |
| HM | Y | Y | Maximum tensile stress criterion & Mohr-Coulomb criterion | U | N | 2D | 0.2×0.2 | COMSOL&MATLAB | Jia et al. (2020) |
| HM | Y | Y | Stress intensity factor K1  Maximum tensile stress criterion & Mohr-Coulomb criterion | Coalbed | N | 2D | 1×1 | COMSOL&MATLAB | Xue et al. (2021) |
| HM | Y | Y | Maximum tensile stress criterion & Mohr-Coulomb criterion | Shale | Bedding planes | 2D | 0.2×0.2 | COMSOL&MATLAB | Zhang et al. (2021) |
| HM | Y | Y | Maximum tensile stress criterion & Mohr-Coulomb criterion | U | Natural fractures | 2D | 100×200 | U | Guo et al. (2022) |
| CZM | HM | N | N | U | U | Natural fractures | 2D | 30×30 | ABAQUS | Song et al. (2019) |
| HM | N | Y | Maximum tensile stress criterion & Mohr-Coulomb criterion | U | N | 2D | 0.2×0.2 | U | Liu et al. (2020) |
| HM | N | Y | U | U | N | 2D | 25×25 | ABAQUS | Cai et al. (2021) |
| HM | N | N | B-K criterion | Shale | N | 3D | R200×H15 | U | Song et al. (2021) |
| HM | Y | Y | U | Coalbed | N | 2D | 0.05×0.05 | U | Yang et al. (2021) |
| PFM | HM | Y | Y | Critical energy release rate criterion | U | N | 2D | 1×1 | U | Ha et al. (2018) |
| HM | Y | N | Critical energy release rate criterion | Shale | Natural fractures | 2D | 1×1 | U | Mollaali et al.(2019) |
| HM | Y | N | Critical energy release rate criterion | U | N | 2D | 4×4 (max) | U | Feng et al. (2021) |
| XEFM | HM | N | N | B-K criterion | Coalbed | N | 2D |  | ABAQUS | Yan et al. (2019) |
| HM | N | N | B-K criterion | Coalbed | N | 2D | 20×10 | ABAQUS & Fluent | Yan et al. (2020) |
| THM | Y | N | Critical energy release rate criterion | Shale | Bedding planes | 2D | 100×100 | U | Luo et al. (2021) |
| HM | N | N | B-K criterion | Coalbed | N | 2D | 20×20 | ABAQUS | Yan et al. (2021) |
| DDM | THM | Y | N | Stress intensity factor K1 | Shale | N | 3D | U | U | Li et al. (2019a) |
| THM | Y | N | Stress intensity factor K1 | U | N | 3D | U | U | He et al. (2020) |
| HM | Y | N | U | U | Natural fractures | 3D | 500×500 | U | Zhao et al. (2021) |
| FDM | THM | N | N | Tensile strength criteria | Tight sandstone | N | 3D | 2000 × 1000 × 2500 | FLAC3D | Liao (2020) |
| PFC | HM | N | Y | Tensile and shear strength criteria | Shale | Natural fractures | 3D | 0.1×0.1×0.1 | PFC3D | Peng et al. (2017) |
| HM | N | Y | Tensile and shear strength criteria | Coalbed | N | 2D | 0.85mm×0.85mm (max) | PFC2D | Zhang et al. (2017b) |
| HM | N | Y | Tensile and shear strength criteria | U | Natural fractures | 2D | 1×1 | PFC2D | Li et al. (2019b) |

Note: DEL- Damage evolution law, CZM- Cohesive zone model, PFM- Phase field method, XFEM- Extended finite element method, DDM- Displacement discontinuity method, FDM- Finite element method, PFC- Particle flow code, Y- Yes, N- No, U- Unknown.

**Table A3** Numerical simulations of proppant transport in SC-CO2 fracturing

|  |  |  |  |  |  |  |  |
| --- | --- | --- | --- | --- | --- | --- | --- |
| Method | | Fracture  propagation | Fracture  geometry | Fracture size (m) | Inlet boundary conditions | Outlet boundary conditions | References |
| Computational  fluid  dynamics | Euler-Euler method | N | Plane fracture | 2.07×0.495×0.009 | Constant mass flows and proppant volume fractions | Atmospheric pressure | Song et al. (2018) |
| N | Plane fracture | 3×0.4×0.01 | Wang et al. (2018a) |
| N | Complex fracture | / | Wang et al. (2018b) |
| N | Plane fracture | 2.4×6×0.006 | Xiao et al. (2018) |
| N | Complex fracture | / | Ge et al. (2019) |
| N | Plane fracture | 3×0.5×0.004 | Zheng et al. (2020a) |
| N | Plane fracture | 60×6×0.02 | Zhou et al. (2020) |
| Euler-Lagrange method | N | Tortuous fracture | / | Xu et al. (2020) |
| N | Plane fracture | 0.7×0.1×0.002 | Zheng et al. (2020b) |
| N | Plane fracture | 0.5×0.15×0.002 | Zheng et al. (2021) |
| Proppant  settlement theory | Combing equilibrium velocity equation with proppant bank increment equation | Y | PKN-type fracture | / | Closure stress | Sun et al. (2018) |
| Y | PKN-type fracture | / | Wang et al. (2019b) |
| Based on the corrected Stokes settlement theory and considering the effects of proppant concentration and fracture wall | Y | Three-dimensional planar fracture | / | Liao (2020) |
| Based on the Dontsov model and considering the effects of proppant concentration and fracture width | Y | PKN-type fracture | / | Wang and Elsworth (2020) |

Note: Y- Yes, N- No

**References**

Bai, J.W., Xiao, C.Y., Mu, C.G., Zheng, L.H., 2019. Study on the wellbore flow for carbon dioxide fracturing. Appl. Sci. 9(9), 1864.

Cai, X., Liu, W., 2021. Hydromechanical-coupled cohesive interface simulation of complex fracture network induced by hydrofracturing with low-viscosity supercritical CO2. Lithosphere 2021 (Special 1), 6689981.

Chen, N.H., 1979. An explicit equation for friction factor in pipe. Ind. Eng. Chem. Fundam. 18(3), 296-297.

Cheng, Y.X., Li, G.S., Wang, H.Z., Shen, Z.H., Cai, C.Z., 2014. Phase control of wellbore fluid during supercritical CO2 jet fracturing. Acta Pet. Sin. 35(6), 1182-1187 (in Chinese).

Churchill.,S.W., 1977. Friction-factor equation spans all fluid-flow regimes. Chem. Eng. 7, 91-92.

Dou, L.B., Li, G.S., Shen, Z.H., Wu, C.F., Bi, G., 2013. Wellbore pressure and temperature prediction model and its affecting factors for CO2 injection wells. Pet. Drill. Tech. 41(1), 76-81 (in Chinese).

Feng, Y.X., Haugen, K., Firoozabadi, A., 2021. Phase‐Field simulation of hydraulic fracturing by CO2, water and nitrogen in 2D and comparison with laboratory data. J. Geophys. Res-Sol. Ea., 126(11), e2021JB022509.

Ge, Q., Ma, X.F., Zhang, S.C., Cao, T., Li, S.H., 2019. Numerical simulation of proppant carrying law of CO2 fluid in complex fractures. J. Xi'an Shiyou Univ., Nat. Sci. Ed. 34(3), 41-48 (in Chinese).

Gong, L., Chen, S.C., Zuo, J.Q., Bai, B., Bai, Z., 2019a. Phase prediction of supercritical carbon dioxide and its application in fracturing oil wellbores. J. Therm. Sci. 28(3), 484-493.

Gong, Q., Xu, Z.G., Wang, M.Q., Qin, J., 2019b. Numerical investigation on wellbore temperature and pressure during carbon dioxide fracturing. Appl. Therm. Eng. 157, 113675.

Guo, J.C., Zeng, J., 2015. A coupling model for wellbore transient temperature and pressure of fracturing with supercritical carbon dioxide. Acta Pet. Sin. 36(2), 203-209 (in Chinese).

Guo, J.C., Zeng, J., Zhang, R., Zhou, C.L., 2015. A dual transient coupling model for wellbore of carbon dioxide injection well. Acta Pet. Sin. 36(8), 976-982 (in Chinese).

Guo, T.K., Zhang, Y.L., Shen, L., et al., 2022. Numerical study on the law of fracture propagation in supercritical carbon dioxide fracturing. J. Petrol. Sci. Eng. 208, 109369.

Ha, S.J., Choo, J., Yun, T.S., 2018. Liquid CO2 fracturing: Effect of fluid permeation on the breakdown pressure and cracking behavior. Rock Mech. Rock Eng. 51(11), 3407-3420.

He, Y.T., Yang, Z.Z., Jiang, Y.F., Li, X., Zhang, Y.Q., Song, R., 2020. A full three-dimensional fracture propagation model for supercritical carbon dioxide fracturing. Energy Sci. Eng. 8(8), 2894-2906.

Jain, A.K., 1976. Accurate explicit equation for friction factor. J. Hydraul. Div. 102(5), 674-677.

Jia, Y.Z., Lu, Z.H., Liu, H., Wang, J.H., Cheng, Y.G., Zhang, X.W., 2020. Fracture propagation and morphology due to non-aqueous fracturing: competing roles between fluid characteristics and in situ stress state. Minerals-Basel. 10(5), 428.

Li, X.J., Li, G.S., Wang, H.Z., et al., 2018. A wellbore flow model and coupling solution for supercritical CO2 fracturing. J. China Univ. Pet., Ed. Nat. Sci. 42(2): 87-94 (in Chinese).

Li, X.G., He, Y.T., Huo, M., Yang, Z.Z., Wang, H.Z., Song, R., 2019a. Simulation of coupled thermal-hydro-mechanical processes in fracture propagation of carbon dioxide fracturing in oil shale reservoirs. Energ. Source. Part A, 1-20.

Li, M.L., Zhang, F.S., Zhuang, L., Zhang, X., Ranjith, P., 2019b. Micromechanical analysis of hydraulic fracturing in the toughness-dominated regime: Implications to supercritical carbon dioxide fracturing. Computat. Geosci. 24(5), 1815-1831.

Liao, J.X., 2020. Development of coupled THM models for reservoir stimulation and geo-energy production with supercritical CO2 as working fluid, 1st ed. Cuvillier Verlag, Gottingen, Germany.

Liu, L.Y., Zhu, W.C., Wei, C.H., Elsworth, D., Wang, J.H., 2018. Microcrack-based geomechanical modeling of rock-gas interaction during supercritical CO2 fracturing. J. Petrol. Sci. Eng. 164, 91-102.

Liu, B.L., Suzuki, A., Ito, T., 2020. Numerical analysis of different fracturing mechanisms between supercritical CO2 and water-based fracturing fluids. Int. J. Rock Mech. Min. 132, 104385.

Luo, Z.F., Cheng, L., Zhao, L.Q., 2021. Numerical simulation and analysis of complex fracture propagation during SC-CO2 fracturing using a thermal-hydro-mechanical coupling model. IOP Conf. Ser.: Earth Environ. Sci. 861(3), 032013.

Lv, X.R., Zhang, S.C., Yu, B.H., et al., 2015. The wellbore temperature test and simulation analysis for liquid carbon dioxide fracturing management. In: SPE/IATMI Asia Pacific Oil & Gas Conference and Exhibition. OnePetro, Nusa Dua, Bali, Indonesia, SPE-176187-MS.

Lyu, X.R., Zhang, S.C., Ma, X.F., Wang, F., Mou, J.Y., 2018a. Numerical investigation of wellbore temperature and pressure fields in CO2 fracturing. Appl. Therm. Eng. 132, 760-768.

Lyu, X.R., Zhang, S.C., Ma, X.F., Wang, F., Mou, J.Y., 2018b. Numerical study of non-isothermal flow and wellbore heat transfer characteristics in CO2 fracturing. Energy 156, 555-568.

Lyu, X.R., Zhang, S.C., He, Y.Y., Zhuo, Z.H., Zhang, C., Meng, Z., 2021. Numerical investigation on wellbore temperature prediction during the CO2 fracturing in horizontal wells. Sustainability-Basel 13(10), 5672.

Mollaali, M., Ziaei-Rad, V., Shen, Y., 2019. Numerical modeling of CO2 fracturing by the phase field approach. J. Nat. Gas Sci. Eng. 70, 102905.

Peng, P.H., Ju, Y., Wang, Y.L., Wang, S.Q., Gao, F., 2017. Numerical analysis of the effect of natural microcracks on the supercritical CO2 fracturing crack network of shale rock based on bonded particle models. Int. J. Numer. Anal. Met. 41(18), 1992-2013.

Song, W.Q., Ni, H.J, Wang, R.H., Sun, B.J., Shen, Z.H., 2017. Pressure transmission in the tubing of supercritical carbon dioxide fracturing. J. CO2. Util. 21, 467-472.

Song, X.Z., Li, G.S., Guo, B., Wang, H.Z., Li, X.J., Lü, Z.H., 2018. Transport feasibility of proppant by supercritical carbon dioxide fracturing in reservoir fractures. J. Hydrodyn. 30(3), 507-513.

Song, X.H., Guo, Y.T., Zhang, J., et al., 2019. Fracturing with carbon dioxide: from microscopic mechanism to reservoir application. Joule 3(8), 1913-1926.

Song, W.Q., Ni, H.J, Tang, P., et al., 2021. Simulation of supercritical carbon dioxide fracturing in shale gas reservoir. J. Therm. Sci. 30(4), 1444-1451.

Sun, B.J., Wang, J.T., Wang, Z.Y., Gao, Y.H., Xu, J.C., 2018. Calculation of proppant-carrying flow in supercritical carbon dioxide fracturing fluid. J. Petrol. Sci. Eng. 166, 420-432.

Wang, H., Touber, S. 1991. Distributed and non-steady-state modelling of an air cooler. Int. J. Refrig. 14(2), 98-111.

Wang, Z.Y., Sun, B.J., Wang, J.T., Hou, L., 2014. Experimental study on the friction coefficient of supercritical carbon dioxide in pipes. Int. J. Greenh. Gas. Con. 25, 151-161.

Wang, M., Wang, H., Li, G., Yang, B., Zheng, Y., Lu, Q., 2018a. Numerical study of proppant transport with supercritical CO2 in fracture. China Pet. Mach. 46(11), 72-78 (in Chinese).

Wang, H.Z., Wang, M., Yang, B., Lu, Q., Zheng, Y., Zhao, H.Q., 2018b. Numerical study of supercritical CO2 and proppant transport in different geometrical fractures. Greenhouse Gases: Sci. Technol. 8(5), 898-910.

Wang, J.T., Sun, B.J., Chen, W.Q., Xu, J.C., Wang, Z.Y., 2019a. Calculation model of unsteady temperature–pressure fields in wellbores and fractures of supercritical CO2 fracturing. Fuel 253, 1168-1183.

Wang, J.T., Wang, Z.Y., Sun, B.J., Gao, Y.H., Wang, X., Fu, W.Q., 2019b. Optimization design of hydraulic parameters for supercritical CO2 fracturing in unconventional gas reservoir. Fuel 235, 795-809.

Wang, J.H., Elsworth, D., 2020. Fracture penetration and proppant transport in gas- and foam-fracturing. J. Nat. Gas Sci. Eng. 77, 103269.

Wu, L., Luo, Z.F., Zhao, L.Q., Zhang, N.L., Yao, Z.G., Jia, Y.C., 2021. Transient temperature‐pressure field model of supercritical CO2 fracturing wellbore with tubing and annulus co-injection. Greenhouse Gases: Sci. Technol. 12(1), 85-102.

Xiao, B., Jiang, T. and Zhang, S., 2018. Numerical simluation on proppant transport of liquid carbon dioxide in vertical fracture. Sci. Technol. Eng. 18(12), 186-190 (in Chinese).

Xu, J.X., Ding, Y.H., Yang, L.F., et al., 2020. Numerical analysis of proppants transport in tortuous fractures of shale gas reservoirs after shear deformation. J. Nat. Gas Sci. Eng. 78, 103285.

Xue, Y., Liu, J., Ranjith, P.G., Liang, X., Wang, S.H., 2021. Investigation of the influence of gas fracturing on fracturing characteristics of coal mass and gas extraction efficiency based on a multi-physical field model. J. Petrol. Sci. Eng. 206, 109018.

Yan, H., Zhang, J.X., Zhou, N., Li, M., 2019. Staged numerical simulations of supercritical CO2 fracturing of coal seams based on the extended finite element method. J. Nat. Gas Sci. Eng. 65, 275-283.

Yan, H., Zhang, J.X., Zhou, N., Li, M., Suo, Y., 2020. Numerical simulation of dynamic interactions between two cracks originating from adjacent boreholes in the opposite directions during supercritical CO2 fracturing coal mass. Eng. Fract. Mech. 223, 106745.

Yan, H., Zhang, J.X., Zhou, N., Wang, Y.B., 2021. Quantitative characterization of crack propagation behavior under the action of stage-by-stage fracturing induced by SC-CO2 fluid. Eng. Fract. Mech. 256, 107984.

Yang, Z.Z., Yi, L.P., Li, X.G., Chen, Y.T., Sun, J., 2018a. Model for calculating the wellbore temperature and pressure during supercritical carbon dioxide fracturing in a coalbed methane well. J. CO2. Util. 26, 602-611.

Yang, Z.Z., Yi, L.P., Li, X.G., Li, Y., Jia, M., 2018b. Phase control of downhole fluid during supercritical carbon dioxide fracturing. Greenhouse Gases: Sci. Technol. 8(6), 1079-1089.

Yang, Z.Z., Yi, L.P., Li, X.G., Han, X.P., Li, Z.C., 2018c. Wellbore temperature and pressure calculation model for supercritical carbon dioxide jet fracturing. Energ. Sources. Part A 41(2), 185-200.

Yang, J.F., Ren, Y.Q., Zhang, D.D, Liu, Y.L., Ma, Z., 2021. Numerical simulation of fracturing in coals using water and supercritical carbon dioxide with potential-based cohesive zone models. Geofluids 2021, 1-14.

Yi, L.P., Jia, M., Li, X.G., Yang, Z.Z., 2019. Transient wellbore temperature and pressure calculation model for supercritical CO2 jet fracturing. Energ. Source. Part A 43(11), 1396-1411.

Zhang, X.X., Wang, J.G., Gao, F., Ju, Y., 2017a. Impact of water, nitrogen and CO2 fracturing fluids on fracturing initiation pressure and flow pattern in anisotropic shale reservoirs. J. Nat. Gas Sci. Eng. 45, 291-306.

Zhang, Y.H., Zhang, Z.k., Sarmadivaleh, M., et al., 2017b. Micro-scale fracturing mechanisms in coal induced by adsorption of supercritical CO2. Int. J. Coal Geol. 175, 40-50.

Zhang, Q., Ma, D., Wu, Y., Meng, F.F., 2018. Coupled thermal−gas−mechanical (TGM) model of tight sandstone gas wells. J. Geophys. Eng. 15(4), 1743-1752.

Zhang, Q., Ma, D., Liu, J.F., Wang, J.H., Li, X.B., Zhou, Z.L., 2019. Numerical simulations of fracture propagation in jointed shale reservoirs under CO2 fracturing. Geofluids 2019, 1-13.

Zhang, Q., Wang, J.H., Gao, Y.F., et al., 2021. CO2-Driven hydraulic fracturing trajectories across a preexisting Fracture. Geofluids 2021, 1-12.

Zhao, H.Q., Wu, K., Huang, Z.W., Xu, Z.M., Shi, H.Z., Wang, H.Z., 2021. Numerical model of CO2 fracturing in naturally fractured reservoirs. Eng. Fract. Mech., 244.

Zheng, W., Song, Z. and Su, W., 2017. To calculate and analyze friction along tubing string during liquid CO2 fracturing. Drill. Prod. Technol. 40, 53-56 (in Chinese).

Zheng, Y., Wang, H.Z., Yang, B., et al., 2020b. CFD-DEM simulation of proppant transport by supercritical CO2 in a vertical planar fracture. J. Nat. Gas Sci. Eng. 84, 103647.

Zheng, Y., Wang, H.Z., Shen, Z.H., Yang, B., Tian, G.H., 2020a. CFD simulation of proppant distribution in a vertical fracture during supercritical CO2 fracturing. In: 54th US Rock Mechanics/Geomechanics Symposium. OnePetro, Golden, Colorado, USA, ARMA-2020-1183.

Zheng, Y., Wang, H.Z., Li, Y.J., et al., 2021. Effect of proppant pumping schedule on the proppant placement for supercritical CO2 fracturing. Petrol. Sci. 19(2), 629-638.

Zhou, Y., Ni, H.J., Shen, Z.H., Wang, M.S., 2020. Study on proppant transport in fractures of supercritical carbon dioxide fracturing. Energ. Fuel. 34(5), 6186-6196.